Short:        scsi v43.46 beta
Author:       Cosmos
Uploader:     cosmos.amiga@gmail.com
Type:         driver/media
Requires:     WB 3.0+ and 68000+
Version:      43.46
Architecture: m68k-amigaos
URL:          http://cosmosamiga.blogspot.com



Improved scsi.device for A600 and A1200

Beta version working fine on ACA630@40, Blizzard 1230@60
and Blizzard 1260@80 with a CF card and FFS.

Need more tests. Please, use a special HD or CF with this
new version : *NOT* on your current setup !


Install :

 - 'Loadmodule scsi.device_43.46_A600_A1200' at the top of
    the StartUp-Sequence

 - Or burn into an eprom, the best way !



scsi.device v43.46 beta 1 (14908 bytes)

 - A600 & A1200 versions unified
 - Debug code removed
 - Read/write function completly rewritten
 - Some subroutines called one time inlined
 - 100% PC relatif
 - Wait states for very old HDs removed
 - Special code for the Conner 20 Mo CP2024 removed
 - 1032 bytes saved


scsi.device v43.45 (15940 bytes)

 - IORequest structure fixed by Chris Hodge
 - Some 48-bit LBA commands fixed By Toni Wilen


